CS350 Module 5-1 Milestone Two Questions

**What is the purpose of the timerCallback() function?**

Handles activities that must occur with every timer tick or loop cycle.

**What does period mean in this context?**

Delay time between each timer tick or loop cycle.

**How does the Timer\_CONTINUOUS\_CALLBACK parameter impact the driver?**

Specifies that the timer loops continuously rather than once.

**What is gpioButtonFxn0() used for?**

Handle what must occur for a GPIO interrupt on CONFIG\_GPIO\_BUTTON\_0.

**What is the purpose of GPIO\_CFG\_IN\_INT\_FALLING?**

Configures button to trigger interrupt for falling edge.